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Specifications

MODEL EA90611 EA901011
Capacity 6 KVA /5400 W 10 KVA /9000 W
INPUT

Rated voltage

208V /220 V/230V /240 Vac

Voltage range

Half load (110 ~ 300) +5 Vac
Full load (160 ~ 300) + 5 Vac

Frequency

40 ~ 70 Hz (auto-sense)

Power factor

=099

Bypass voltage range

160V ~ rated output voltage +32V

OUTPUT

Voltage 208V /220 V /230 V/ 240 Vac (settable via LCD)

Voltage regulation 1%

Frequency 45 ~ 55 Hz or 55 ~ 65 Hz (synchronized range); 50 /60 Hz_+ 0.2 Hz (battery mode)
Waveform Sinusoidal

Crest factor 31

Harmonic distortion < 2% (linear load); = 5% (non~linear load)

Transfer time oms

Overload capability

105% ~ 125%: transfer to bypass in 3 mins;
125% ~ 150%: transfer to bypass in 30's;
> 150%: transfer to bypass in 100 ms

EFFICIENCY

Mains mode = 92%
Battery mode =91%
ECO mode = 98%

BATTERIES
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6KVA ~ 10KVA
PFO0.9

@ High frequency and true double-conversion
@ DSP digital control technology

@ Input power factor correction (PFC)

® Wide input voltage range (110V ~ 300V)

® Output power factor 0.9

@ Cold start

@ Auto sensing frequency

@® ECO mode operation for energy saving

@ Selectable output voltage via LCD

® 50 Hz /60 Hz frequency conversion mode available
@ Selectable battery low voltage via LCD

® Power-on self test

@ Advanced battery management (ABM)

@ Short circuit and overload protection

@ Automatic charging in OFF mode

® Fan speed auto control when loads varies
@ Standard RS232 communication port

@ Optional USB / SNMP communication port
@ Optional emergency power off (EPO)

@ Optional extension battery bank

@ Optional built-in isolation transformer

@ Optional manual bypass

@ Optional N+X redundancy parallel
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DC voltage 192V
Inbuilt battery of standard model 16 x 7 Ah 16 x 9 Ah
Charging current Standard model 1A

Long time model 1A/3A/5A/8A
Recharge time 8h
ALARMS
Utility failure 4s per beep
Low battery 1s per beep
Overload 15 twice beep
UPS fault Long beep
COMMUNICATIONS

RS232 (standard), USB (optional)

Supports Windows* 98 / 2000 / 2003 / XP / Vista / 2008 / Windows" 7 /8 / 10

SNMP (optional)

Power management from SNMP manager and web browser

OTHERS
Humidity 20 ~90% RH @ 0 ~ 40°C (non-condensing)
Noise level = 55dB (1m)

Dimensions (W x D x H) (mm)

262 x 514 x 455 (H), 262 x 514 x 735 (S)

Packaged dimensions (W x D x H) (mm)

365 x 605 x 610 (H), 390 x 625 x 937 (S)

Netweight (kg) 22.1(H).64.1(S) 22.8(H).70.8(S)
Gross weight (kg) 25.2(H), 72.2(S) 25.9 (H), 78.9(S)
@Derato capacity to 70% in CUCF mado and 10 90% when the output voltaga is adjusted to 208Vac. ® All specifications subject to change without notice.

5 moans standard model, Hmeans long time model

@ Custom-made specifications are acceptable.
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1.AC Input

2. Modem/Tel/Fax

3.DC Input

4. Outlet

5.Fan

6.RS232

7. USB (optional)

8. EPO (optional)

9. Manual Bypass (optional)
10. SNMP/AS400 (optional)
11. Breaker

12. Parallel Card (optional)
13. BAT_NTC (optional)





