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MODEL

ZTY Three Phase

VA Rating 3KVA BKVA 10KVA 15KVA 20KVA 30KVA
INPUT

Phase Three Phase+N+GND

Voltage Range Line Voltage 277Vac-433Vac

OUTPUT

Voltage 380V

Voltage Precision < +3%

Frequency 50/60Hz

Over-voltage Protection Output Voltage 250V + 5V

Low-voltage Protection Output Voltage 183V +5V

Efficiency =96%

OTHERS

Display Model LED /METER

Input/Output Device Terminal

Waveform Distortion No Affixation Waveform Distortion

Response Time (+10% Varies) <1s

Insulation Resistance =2MQ

Anti-electricy Intension Low Frequency Sine Voltage 1500V Take 1 minute No Rout and Camber phenomena
Ambient Temperature 0°C-40C

Relative Humidity <95%

Working Continue

Dimension(WxDxH)mm 200x480x395 330x350x702 330x380x752 530x400x732
Net Weight(kg) 145 35 [ 37 51 | 58 95
Packing(WxDxH)mm 260x555x505 460x435x790 555x420x840 635x500x830
Gross Weight(kg) 16.8 37.6 [ 40 54.2 [ 61.6 105
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ZTY series high accuracy fully automatic AC stabilized Power Supply is a key series of our stabilizing products. It mainly
consists of auto—transformer, servo motor, automatic control circuit. When the utility is not stable or the load fluctuates, the
automatic control circuit modifies the control output according to the input voltage change of power supply, with driving the
servo motor, and then the servo motor adjusting the carbon brush of auto-transformer to regulate the output voltage at its
rating and remain stable.

All our products are manufactured in ISO-9001:2000 certified facilities and environmentally friendly. Zero tolerance in our
Quality Assurance tests at all levels of production continues to eliminate failures in the field. We presently enjoy "o" stabilized
power supply failure in the field and DOA's(Dead on Arrival) are non—existent.
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MODEL ZTY Single Phase

VA Rating 0.5KVA 1KVA 2KVA 3KVA S5KVA 10KVA 15KVA 20KVA 30KVA
INPUT

Phase Single Phase + N+ GND

Voltage Range 160Vac-250Vac

OUTPUT

Voltage 220V

Voltage Precision < +3%

Frequency 50/60Hz

Over-voltage Protection Output Voltage 250V + 5V

Low-voltage Protection Output Voltage 183V +5V

Efficiency =96%

OTHERS

Display Model LED/METER

Input/Output Device Optional Plug; Socket/Terminal

Waveform Distortion No affixation Waveform Distortion

Response Time (+10% Varies) <1s

Insulation Resistance =2MQ

Anti-electricy Intension Low Frequency Sine Voltage 1500V Take 1 minute No Rout and Camber phenomena

Ambient Temperature 0°C-40°C

Relative Humidity <95%

Working Continue

Dimension(WxDxH)mm 150x247x144 150x247x200| 150x285x260 | 175x360x305| 220x485x430 330x370x612 530x400x732
Net Weight(kg) 4.3 ‘ 4.8 8.2 9.5 15.2 31 53 ‘ 59 91
Packing(WxDxH)mm 235x360x235 235x360x290 | 230x395x350 [278x470x415| 280x555x495 430x500x690 635x500x830
Gross Weight(kg) 5.3 10.1 15.9 32 56 61.3 94.5
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